<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="8.382" y2="0" width="0" layer="20"/>
<wire x1="8.382" y1="0" x2="8.382" y2="2.286" width="0" layer="20"/>
<wire x1="8.382" y1="2.286" x2="39.116" y2="2.286" width="0" layer="20"/>
<wire x1="39.116" y1="2.286" x2="39.116" y2="0" width="0" layer="20"/>
<wire x1="39.116" y1="0" x2="47.625" y2="0" width="0" layer="20"/>
<wire x1="47.625" y1="0" x2="47.625" y2="26.416" width="0" layer="20"/>
<wire x1="47.625" y1="26.416" x2="45.593" y2="26.416" width="0" layer="20"/>
<wire x1="45.593" y1="26.416" x2="45.593" y2="37.592" width="0" layer="20"/>
<wire x1="45.593" y1="37.592" x2="47.625" y2="37.592" width="0" layer="20"/>
<wire x1="47.625" y1="37.592" x2="47.625" y2="47.625" width="0" layer="20"/>
<wire x1="47.625" y1="47.625" x2="0" y2="47.625" width="0" layer="20"/>
<wire x1="0" y1="47.625" x2="0" y2="0" width="0" layer="20"/>
<text>D1</text>
<text>15A Max</text>
<text>PD15</text>
<text>R1</text>
<text>R2</text>
<text>Q1</text>
<text>-</text>
<text>+</text>
<text>-</text>
<text>+</text>
<text>-</text>
<text>+</text>
<text>LED</text>
<text>Rmt On</text>
<text>R3</text>
<text>Q2</text>
<text>Q3</text>
<text>1.575 Inches</text>
<text>1.875 Inches</text>
<text>Batt</text>
<text>+</text>
<text>-</text>
<text>(C) 2016, Demand Peripherals, Inc.</text>
<text>Rev 16A</text>
<text>1.575 Inches</text>
<text>1.875 Inches</text>
<text>Off</text>
<text>On</text>
</plain>
<libraries>
<library name="DP">
<packages>
<package name="FIDUCIAL">
</package>
<package name="DPI-2">
<description>Demand Peripherals Symbol #2</description>
</package>
<package name="LETTER_P">
<description>&lt;b&gt;FRAME&lt;/b&gt; LETTER portrait</description>
</package>
</packages>
</library>
<library name="dpi-conn">
<packages>
<package name="HDR-2X1">
<description>2x1 PIN HEADER on 0.1 inch centers</description>
</package>
<package name="DC-BARREL-JACK-55MM">
<description>&lt;b&gt;5.5 mm DC BARREL JACK&lt;/b&gt;&lt;p&gt;
Source:CUI PJ-102AH</description>
</package>
<package name="AUTO_FUSE-V">
<description>Spade</description>
</package>
<package name="TBLK-5.08-X2">
<description>&lt;b&gt;Terminal Block, 5.08mm, x2&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="dpi-transic">
<packages>
<package name="DPACK_TO-252">
<description>D-Pack TO-252</description>
</package>
</packages>
</library>
<library name="dpi-passive">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="dpi-diopto">
<packages>
<package name="LED5MM">
<description>LED, 5 mm, round</description>
</package>
<package name="SOD123">
</package>
</packages>
</library>
<library name="dpi-swsens">
<packages>
<package name="SWITCH-PADDLE">
</package>
<package name="TOGGLE_SPDT_PC">
<description>SPDT TOGGLE SWITCH</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="dpi-passive" package="R0603" value="5K">
<attribute name="VENDOR" value="Digikey"/>
<attribute name="VENDOR-PART-NUM" value="311-4.99KHRTR-ND"/>
</element>
<element name="D1" library="dpi-diopto" package="SOD123" value="12V">
<attribute name="VENDOR" value="Digikey"/>
<attribute name="VENDOR-PART-NUM" value="BZT52C1213-FDICT-ND"/>
</element>
<element name="J1" library="dpi-conn" package="DC-BARREL-JACK-55MM" value="Barrel-5.5mm">
<attribute name="VENDOR" value="Digikey"/>
<attribute name="VENDOR-PART-NUM" value="CP-102AH-ND"/>
</element>
<element name="R2" library="dpi-passive" package="R0603" value="1K">
<attribute name="VENDOR" value="Digikey"/>
<attribute name="VENDOR-PART-NUM" value="311-1.00KHRTR-ND"/>
</element>
<element name="FUSE" library="dpi-conn" package="AUTO_FUSE-V" value="FUSEAUTO">
<attribute name="VENDOR" value="Digikey"/>
<attribute name="VENDOR-PART-NUM" value="3522-2K-ND"/>
</element>
<element name="U$12" library="DP" package="FIDUCIAL" value=""/>
<element name="Q1" library="dpi-transic" package="DPACK_TO-252" value="FET_DPAK_P">
<attribute name="VENDOR" value="Digikey"/>
<attribute name="VENDOR-PART-NUM" value="785-1103-1-ND"/>
</element>
<element name="Q2" library="dpi-transic" package="DPACK_TO-252" value="FET_DPAK_P">
<attribute name="VENDOR" value="Digikey"/>
<attribute name="VENDOR-PART-NUM" value="785-1103-1-ND"/>
</element>
<element name="Q3" library="dpi-transic" package="DPACK_TO-252" value="AOD409">
<attribute name="VENDOR" value="Digikey"/>
<attribute name="VENDOR-PART-NUM" value="785-1103-1-ND"/>
</element>
<element name="LED1" library="dpi-diopto" package="LED5MM" value="LED-5MM-GRN">
<attribute name="VENDOR" value="Digikey"/>
<attribute name="VENDOR-PART-NUM" value="160-1852-ND"/>
</element>
<element name="R3" library="dpi-passive" package="R0603" value="100K">
<attribute name="VENDOR" value="Digikey"/>
<attribute name="VENDOR-PART-NUM" value="311-100KHRTR-ND"/>
</element>
<element name="U$3" library="DP" package="FIDUCIAL" value=""/>
<element name="U$4" library="DP" package="FIDUCIAL" value=""/>
<element name="U$8" library="DP" package="DPI-2" value=""/>
<element name="SW2" library="dpi-swsens" package="SWITCH-PADDLE" value="SWITCH-PADDLE">
<attribute name="VENDOR" value="DPI"/>
<attribute name="VENDOR-PART-NUM" value="DPI-paddle-switch"/>
</element>
<element name="TOGGLE-SWITCH" library="dpi-swsens" package="TOGGLE_SPDT_PC" value="B12EH">
<attribute name="VENDOR" value="Digikey"/>
<attribute name="VENDOR-PART-NUM" value="CKN1454-ND"/>
</element>
<element name="U$1" library="DP" package="LETTER_P" value="DP_FRAME_P"/>
<element name="CN1" library="dpi-conn" package="HDR-2X1" value="">
<attribute name="VENDOR" value="Mouser"/>
<attribute name="VENDOR-PART-NUM" value="571-6404562"/>
</element>
<element name="CN2" library="dpi-conn" package="TBLK-5.08-X2" value="">
<attribute name="VENDOR" value="Digikey"/>
<attribute name="VENDOR-PART-NUM" value="ED2609-ND"/>
</element>
<element name="CN3" library="dpi-conn" package="TBLK-5.08-X2" value="">
<attribute name="VENDOR" value="Digikey"/>
<attribute name="VENDOR-PART-NUM" value="ED2609-ND"/>
</element>
<element name="CN4" library="dpi-conn" package="TBLK-5.08-X2" value="">
<attribute name="VENDOR" value="Digikey"/>
<attribute name="VENDOR-PART-NUM" value="ED2609-ND"/>
</element>
<element name="CN5" library="dpi-conn" package="TBLK-5.08-X2" value="">
<attribute name="VENDOR" value="Digikey"/>
<attribute name="VENDOR-PART-NUM" value="ED2609-ND"/>
</element>
</elements>
<signals>
<signal name="V+">
<contactref element="Q1" pad="4"/>
<contactref element="Q3" pad="4"/>
<contactref element="Q2" pad="4"/>
<contactref element="R2" pad="2"/>
<contactref element="CN2" pad="2"/>
<contactref element="CN4" pad="2"/>
<contactref element="CN3" pad="2"/>
</signal>
<signal name="BATT+">
<contactref element="FUSE" pad="LS@1"/>
<contactref element="FUSE" pad="LS@2"/>
<contactref element="CN5" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R1" pad="2"/>
<contactref element="Q1" pad="1"/>
<contactref element="Q3" pad="1"/>
<contactref element="Q2" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="ON+">
<contactref element="R1" pad="1"/>
<contactref element="TOGGLE-SWITCH" pad="2"/>
<contactref element="SW2" pad="1"/>
<contactref element="CN1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="3"/>
<contactref element="LED1" pad="C"/>
<contactref element="TOGGLE-SWITCH" pad="3"/>
<contactref element="SW2" pad="2"/>
<contactref element="CN1" pad="2"/>
<contactref element="CN2" pad="1"/>
<contactref element="CN4" pad="1"/>
<contactref element="CN3" pad="1"/>
<contactref element="CN5" pad="1"/>
</signal>
<signal name="FUSE+">
<contactref element="FUSE" pad="RS@3"/>
<contactref element="FUSE" pad="RS@4"/>
<contactref element="Q1" pad="3"/>
<contactref element="Q2" pad="3"/>
<contactref element="Q3" pad="3"/>
<contactref element="D1" pad="C"/>
<contactref element="R3" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$4">
</signal>
<signal name="MOUNT">
</signal>
<signal name="N$5">
</signal>
</signals>
</board>
</drawing>
</eagle>
